>> trying 32MB allocation :failed
>> trying 24MB allocation : failed
>> trying 16MB allocation : OK!!
> cbx=2
> cby=480
> assemdebug r11= 2
> Cart selected :
>>\CF Card\½´·Î´ëD\SRWD.gba
>> Cart size : 0x800000
>> CART. path = \CF Card\½´·Î´ëD
>> Load cart. OK!
>> Loaded cart : \CF Card\½´·Î´ëD\SRWD.gba
> Cart selected :
>>\CF Card\½´·Î´ëD\SRWD.gba
>> Cart size : 0x800000
>> CART. path = \CF Card\½´·Î´ëD
>> Load cart. OK!
>> Loaded cart : \CF Card\½´·Î´ëD\SRWD.gba
>> State file is rel.060324
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> TBit = 0
>> Load state file OK
>> r15 = 0000001C
>> refresh tick = 272
>> gba.timer0 = 0
>> gba.dma0 = 0
>> 0 / 0 / 0 / 0 / 1 / 0
>> Update state with HW-reg OK
>> Update sound state OK
>> system resumed
>> State file is rel.060324
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> TBit = 0
>> Load state file OK
>> r15 = 0000001C
>> refresh tick = 272
>> gba.timer0 = 0
>> gba.dma0 = 0
>> 0 / 0 / 0 / 0 / 1 / 0
>> Update state with HW-reg OK
>> Update sound state OK
>> system resumed
>> State file is rel.060324
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> TBit = 0
>> Load state file OK
>> r15 = 0000001C
>> refresh tick = 272
>> gba.timer0 = 0
>> gba.dma0 = 0
>> 0 / 0 / 0 / 0 / 1 / 0
>> Update state with HW-reg OK
>> Update sound state OK
>> system resumed
>> State file is rel.060324
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> intr. vector = 00100EE8
>> sw intr. vector = 00100ED8
>> TBit = 0
>> Load state file OK
>> r15 = 0000001C
>> refresh tick = 272
>> gba.timer0 = 0
>> gba.dma0 = 0
>> 0 / 0 / 0 / 0 / 1 / 0
>> Update state with HW-reg OK
>> Update sound state OK
>> system resumed
>> system resumed
>> Debug r11=1052964
